**Practicum 4.1.1: DHCP installeren**

**Installatie server role DHCP Server**

Server role DHCP Server geïnstalleerd: Ja.

Gelijk beheertools mee geïnstalleerd: Ja.

Groepen DHCP Administrators en DHCP Users

aan laten maken: Ja.

Gebruikte credentials: ?

Geautoriseerd: Ja

**Configureren**

**ope** Scope Name: PFScopePFSV1

Start IP Address: 192.168.101.31

End IP Address: 192.168.101.130

Subnet Mask: 255.255.255.0

**Exclusions**

Start IP Address: 192.168.101.81

End IP Address: 192.168.101.130

**Lease duur**

Dagen: 7

**DHCP Options**

Router (Default Gateway): 192.168.101.11

Parent name: PoliForma.nl

IP-adres van de DNS-servers: 192.168.101.11/192.168.101.12

WINS: Ja

Geactiveerd: Ja

**Practicum 4.2.1: Scope; containers en eigenschappen**

**Plaats van de DHCP-bestanden**

Database path: C:\Windows\system32\dhcp

Backup path: C:\Windows\system32\dhcp\backup

**De DHCP Scope PFScopePFSV1**

**Address Pool**

Start IP Address: 192.168.101.31

End IP Address: 192.168.101.81

**Scope Options**

Option Value

003 Router 192.168.101.11

006 DNS Server 192.168.101.11, 192.168.101.12

015 DNS Domain Name PoliForma.nl

**Scope eigenschappen**

**Samenwerking met DNS**  X Enable DNS dynamic updates according to the

settings below:

X Dynamically update DNS A and PTR records only if requested by the DHCP clients

⭘ Always dynamically update DNS A and PTR records

X Discard A and PTR records when lease is deleted

🞎 Dynamically update DNS A and PTR records for DHCP clients that do not request updates